TOWN OF JOHNSTOWN

PROJECT DESCRIPTION

Base Bid

1. Indian Road from Montgomery County Line to County Highway 116A. Cold in place recycle and top course same year.

Length Width Depth Material

1.27 Miles 21 Ft. 2 in. compacted 6f

1. Wemple Road from Watershed Road 1.5 Miles inward. 1.5 Miles Binder

Length Width Depth Material

1.5 Miles 20 Feet 2 in. compacted Type 3 Binder

1. North Bush Road from Caroga Town Line 1.5 miles in to culvert crossing.

Length Width Depth Material

1.5 Miles 20 Feet 2 in. compacted 6f

The Town of Johnstown Highway Department will do all the necessary work to prepare the roads for paving, including the cleaning of all pavement involved and boxing out for Binder areas. Contractors are to clean all pavement areas prior to and during rebate and paving process.

Contractor responsible for flagging, maintenance and protection of traffic control and rebates at all driveways and intersections.

All Roads are to have Tack Coat.

Shim Course Type #3 as needed.

The Town of Johnstown reserves the right to add or decrease project tonnage based on monies available, and to reject any and/or all bids at its discretion.

Award will be based on the lowest base bid received.

Any questions about the bid or specifications can be answered by Lucas Hart, Town of Johnstown Highway Superintendent at

518-775-9803.